# Amadee-18-ScanMars

Last modified by jflunger on 2018/08/16 13:13
Export
Office Formats
Export as PDF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

### Details

Acronym | ScanMars
Description | ScanMars is a ground penetrating radar which detects variations in dielectric properties of the ground.
Principal Investigator (PI) | Maurizio Ercoli
Organisation | University of Perugia, Italy

### Summary

ScanMars instrument will image the subsurface of the study area by means of 2d transects of tens of meters. Depending on the available time for the experiment we can extend the observations to a 3D volume.

### Objectives

The setting of the subsurface of the study area represents an important element in the reconstruction of the geologic evolution of the study area. Data will be georeferenced so it can be integrated with the observation of the other instruments.

### Experiment Data

Date | Files
--- | ---
03-Feb-2018 | 2 'sgy' files
08-Feb-2018 | 1 'sgy' file
09-Feb-2018 | 1 'sgy' file
13-Feb-2018 | 4 'sgy' files
18-Feb-2018 | 1 'sgy' file and a note
20-Feb-2018 | 4 'sgy' files, 12 'jpg' files and 3 'flac' audio files
22-Feb-2018 | 4 'sgy' files and 23 'jpg' files
24-Feb-2018 | 4 'sgy' files and 19 'jpg' files
25-Feb-2018 | 2 'sgy' files and a report

### Additional Publications

References | Access
--- | ---
Frigeri, A., Ercoli, M., Pauselli, C.,& Groemer, G. (2018). The ScanMars radar onboard AMADEE-18 analog mission to Mars. EPSC 2018. | Full Tex

0
Tags:
Created by Barry Bishop on 2018/02/11 10:33

- Attachments (1)

Copyright 2018 - Österreichisches Weltraum Forum. All rights reserved.
Contact us - Privacy Policy